Structured Review of Trade Multiskilling Duties for a Plasterer
1. Core Plastering Responsibilities
· Skim coating, bonding, patch plastering, and full wall/ceiling preparation.
· Application of plasterboard including dot and dab or fixed systems.
· Repairs to internal walls and ceilings following water ingress or structural movement.
· Ensuring high-quality finishes meeting organisational standards.
2. Multiskilling Duties for Plasterers
· Injection DPC.
· Patch pointing up to 1 square metre at low level.
· Ceramic wall tiling – remove, renew, replace, and apply silicone sealant.
· Remove and replace thermoplastic floor tiles.
· Refix/renew quarry tiles to floors up to 1 square metre, steps, or cills.
· Mastic pointing to doors, windows, and sanitary fittings.
· Renew or Refit Timber skirtings boards and architraves in conjunction with other work - All types .
· Clean out guttering, valley gutters, and rainwater pipes.
· Repair leaks to gutters including replacement of fittings.
· Renew/realign gutters and downspouts including brackets and supports.
· Refix soil vent pipes including brackets and supports.
· Refix/renew timber floorboards.
· Timber studding to form walls and noggins between joists or studs to receive plasterboard.
· Fit or replace air bricks, sleeves, and ventilators to walls.
· Patch repairs to internal brick and blockwork walls up to 1 square metre, including bricking up fireplaces.
· Remove and refit central heating radiators including brackets, refilling, and testing.
· Remove and refix access panels and ducts including bath panels.
· Remove and re-hang internal doors.
· Renew or adjust ironmongery to doors and gates including hinges, latches, locks, and furniture.
· Carry out decoration/painting work on newly fitted or repaired items.
· Take out and refix kitchen units including sink unit.
· Clean out gulleys.
· To undertake any training and carry out other duties, including works identified in the void standard, commensurate with the role.

3. Health & Safety Requirements
· Compliance with RAMS and safe working practices.
· Correct use of PPE including eye, respiratory, and hand protection.
· Safe handling and disposal of plaster, bonding agents, and adhesives.
· Asbestos awareness and correct escalation if suspected materials are identified.
4. Customer Service & Communication
· Clear communication regarding work requirements and expected timelines.
· Respectful conduct in occupied properties.
· Accurate recording of job notes, follow-on requirements, and material usage.
5. Quality Standards & Performance
· High-quality finish to all plastered, repaired, or decorated surfaces.
· Right-first-time approach to reduce follow-on repairs.
· Consistent achievement of organisational quality, productivity, and compliance expectations.
